Information regarding the files in this directory
=================================================

General Files
*************

Apochromat
~~~~~~~~~~

Trying to open this file causes an error such as "Can't open File" This is 
because a particular glass/glass catalog is missing.


POP setting (.CFG) files
~~~~~~~~~~~~~~~~~~~~~~~~

RESET_SETTINGS_POP_IRR.CFG
--------------------------
most basic settings file (created using "reset" on "LENS.ZMX" lens file) to 
return irradiance data in POP analysis


RESET_SETTINGS_POP_PHASE.CFG
----------------------------
most basic settings file (created using "reset" on "LENS.ZMX" lens file) to 
return phase data in POP analysis


RESET_SETTINGS_FFTPSF.CFG
-------------------------
most basic settings file (created using "reset" on "LENS.ZMX" lens file) to 
return FFT PSF analysis


RESET_SETTINGS_FFTPSFCS.CFG
---------------------------
most basic settings file (created using "reset" on "LENS.ZMX" lens file) to 
return FFT PSF Cross section analysis


RESET_SETTINGS_HUYGENSPSF.CFG
-----------------------------
most basic settings file (created using "reset" on "LENS.ZMX" lens file) to 
return Huygens PSF analysis


RESET_SETTINGS_HUYGENSPSFCS.CFG
-------------------------------
most basic settings file (created using "reset" on "LENS.ZMX" lens file) to 
return Huygens PSF Cross section analysis

RESET_SETTINGS_FFTMTF.CFG
-------------------------
most basic settings file (created using "reset" on "LENS.ZMX" lens file) to 
return FFT MTF analysis

RESET_SETTINGS_HUYGENSMTF.CFG
-----------------------------
most basic settings file (created using "reset" on "LENS.ZMX" lens file) to 
return FFT MTF analysis

RESET_SETTINGS_IMGSIM.CFG
-------------------------
most basic settings file (created using "reset" on "LENS.ZMX" lens file) to 
return image simulation analysis

Unit-test files
***************

Fiber Coupling settings (.CFG) files for unit-tests
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

Fiber Coupling_POPunittest.CFG
------------------------------
The original (unmodified) POP settings for Fiber Coupling.ZMX file. In this
setting, the display data type is Irradiance, fiber coupling integral is
checked, beam is a Gaussian TEM00.

Fiber Coupling_POPunittest_Irradiance.CFG
-----------------------------------------
POP settings to return Irradiance data, the ``surf to beam`` is set to -3 m.
This settings doesn't affect the irradiance, but changes the phase and thus
the coupling efficiency. 

Fiber Coupling_POPunittest_Phase.CFG
------------------------------------
POP settings to return Phase data, the ``surf to beam`` is set to -3 m.
This settings doesn't affect the irradiance, but changes the phase and thus
the coupling efficiency.

Fiber Coupling_POPunittest_NoFiberCompute.CFG
---------------------------------------------
POP settings to return Irradiance data. The "computer fiber integral" option
is checked-OFF in this settings file.
