# 3D Model
This file features notes about different parts of the aircraft, for 3d modelling purpose, along with reference.

* LANDING GEAR (ref. [1] p.8-17 and ref. [7]):
	* Nose Landing Gear: Wheel is a Goodyear 6.00-6 / 8 PRTT
		Outside diameter:	16.8 - 17.5 in ( 0.427 - 0.445 m )  
		Width:			6 in ( 0.152 m )
